Motor info:

A2212 motor:  
KV: 1000 Max  
Efficiency: 80%  
Max Efficiency Current: 4-10A (>75%)  
Current Capacity: 12A/ 60s  
No Load Current @ 10V: 0.5A  
No. Of Cells: 2-3 Li-Poly  
Motor Dimensions: 27.5\* 30mm  
Shaft Diameter: 3.17mm  
30A brushless ESC:  
Output: Continuous 30A  
Input Voltage: 2-4 cells lithium battery or 5-12 cells NiCd/NIMh battery.  
BEC: 2A / 5V (Linear mode).  
1045 Propellers:  
Diameter of Shaft: 6.0mm  
Adjustable by hole adapter (3mm, 3.2mm, 4mm, 5mm, 6mm, 6.35mm, 7.95mm)  
Thickness of center: 9.7mm  
Weight: 15 gram / pair  
Recommended wheelbase: 550mm - 700mm